IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-07-26T10:44:52"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190108_1515(x64) - Exporter 19.2.1.1 - Alternate UI 19.2.1.1"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "U386625" of Organization (no name given)
  Owner history of Person "U386625" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AVDO_DN20_Straight_External_003L6025" | object type "AVDO_DN20_Straight_External_003L6025" | names: "AVDO_DN15-25_Straight_External_RFA:AVDO_DN20_Straight_External_003L6025:932647" | material: materials ("Ms 58 (CuZn 39 Pb 2)", "Paper", "Plastic - Danfoss - Black") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon

Types
  IFCVALVETYPE "AVDO_DN20_Straight_External_003L6025" | 1 occurrence | material: materials ("Ms 58 (CuZn 39 Pb 2)", "Paper", "Plastic - Danfoss - Black") | property sets: Pset_AB-QM

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Danfoss" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "AVDO_DN20_Straight_External_003L6025" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_AB-QM | properties | on 1 type object
    Connection = "ISO 228/1" (IFCTEXT)
    Description = "AVDO DN20 Straight External thread" (IFCTEXT)
    IfcExportAs = "IfcValveType" (IFCTEXT)
    IfcExportType = "Valve-AVDO" (IFCTEXT)
    Manufacturer = "Danfoss" (IFCTEXT)
    Max Differential Pressure = "0.5 bar" (IFCTEXT)
    Max Flow Temperature = "120 C" (IFCTEXT)
    Max Leakage at Closed Valve = "50 l/h" (IFCTEXT)
    Model = "003L6025" (IFCTEXT)
    Operation Pressure = "PN 10" (IFCTEXT)
    Setting Range = "0.05 - 0.5 bar" (IFCTEXT)
    URL = "https://assets.danfoss.com/documents/DOC008986402861/DOC008986402861.pdf" (IFCTEXT)
    Valve Body Material = "Ms 58 (CuZn 39 Pb 2)" (IFCTEXT)