IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "RevitIdentifiers [VersionGUID: bf1c0c5a-7a10-42ef-b00f-f43ffa5c4a85, NumberOfSaves: 16]"
Time stamp: "2024-06-04T10:59:06+01:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "Autodesk Revit 23.1.30.97 (ENG) - IFC 23.3.1.0"
Application: "Autodesk Revit 2023 (ENG)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENG)"

People and organizations
  Person "pavlov_m" of Organization (no name given)
  Owner history of Person "pavlov_m" of Organization (no name given) | application "Autodesk Revit 2023 (ENG)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENG)" | change NOCHANGE | created 1701350568 (2023-11-30T13:22:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCACTUATORTYPE "TWA-K_RFA:TWA-K_230V_NC/S_0.95m_088H3105" | object type "TWA-K_RFA:TWA-K_230V_NC/S_0.95m_088H3105" | names: "TWA-K_RFA:TWA-K_230V_NC/S_0.95m_088H3105:646819" | material: materials ("Danfoss Plastic White", "Danfoss Plastic Black") | property sets: Pset_QuantityTakeOff, Danfoss

Types
  IFCACTUATORTYPE "TWA-K_RFA:TWA-K_230V_NC/S_0.95m_088H3105" | 1 occurrence | material: materials ("Danfoss Plastic White", "Danfoss Plastic Black") | property sets: Pset_ManufacturerTypeInformation

Property sets
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    Reference = "TWA-K_230V_NC/S_0.95m_088H3105" (IFCIDENTIFIER)
  Danfoss | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    Body Material = "Danfoss Plastic White" (IFCLABEL)
    Cable Length = 950.00000000000011 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing and Opening Time = "3 min" (IFCTEXT)
    Connection = "M30 x 1.5" (IFCTEXT)
    Control Input Signal = "On/Off" (IFCTEXT)
    Description = "Thermal Actuator" (IFCTEXT)
    Function = "NC (with end-switch)" (IFCTEXT)
    H = 63.850000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    IfcExportAs = "IfcActuatorType" (IFCTEXT)
    IfcExportType = "TWA-K" (IFCTEXT)
    L = 40.5 (IFCLENGTHMEASURE) [MILLI METRE]
    LOD 200 = FALSE (IFCBOOLEAN)
    LOD 350 = TRUE (IFCBOOLEAN)
    Manufacturer = "Danfoss" (IFCTEXT)
    Max Ambient Temperature = "60 °C" (IFCTEXT)
    Min Ambient Temperature = "0 °C" (IFCTEXT)
    Model = "088H3105" (IFCTEXT)
    Model Type = "TWA-K_230V_NC/S_0.95m" (IFCTEXT)
    OmniClass Number = "23.65.55.14.17" (IFCTEXT)
    OmniClass Title = "Adjusting/Controlling Valves for Liquid Services" (IFCTEXT)
    Power = 2. (IFCPOWERMEASURE) [WATT]
    URL = "https://store.danfoss.com/en/Climate-Solutions-for-heating/Hydronic-floor-heating/Thermal-actuators/c/4218?q=%3Arelevance%3Adanfoss_producttypehierarchydesc%3ATWA-K%3Adanfoss_a1195338584%3AA1195_338584aed5a1b84b32adae464f9231043fe7cb&page=0&pageSize=10" (IFCTEXT)
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    W = 40.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Weight = 0.13600000000000001 (IFCMASSMEASURE) [KILO GRAM]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Danfoss" (IFCLABEL)