IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "RevitIdentifiers [VersionGUID: d4e43186-8d17-40ea-ab9c-e0786ffb1ec4, NumberOfSaves: 17]"
Time stamp: "2024-10-14T10:50:51+01:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "Autodesk Revit 23.1.30.97 (ENG) - IFC 23.3.1.0"
Application: "Autodesk Revit 2023 (ENG)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENG)"

People and organizations
  Person "U373195" of Organization (no name given)
  Owner history of Person "U373195" of Organization (no name given) | application "Autodesk Revit 2023 (ENG)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENG)" | change NOCHANGE | created 1722849268 (2024-08-05T09:14:28Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Supercal 5_RFA:Supercal 5_1l/p_230V_M-Bus_187F8309" | object type "Supercal 5_RFA:Supercal 5_1l/p_230V_M-Bus_187F8309" | names: "Supercal 5_RFA:Supercal 5_1l/p_230V_M-Bus_187F8309:627420" | material: "Danfoss Plastic White" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Danfoss

Types
  IFCVALVETYPE "Supercal 5_RFA:Supercal 5_1l/p_230V_M-Bus_187F8309" | 1 occurrence | material: "Danfoss Plastic White" | property sets: Pset_ManufacturerTypeInformation

Property sets
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "Supercal 5_1l/p_230V_M-Bus_187F8309" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "Supercal 5_1l/p_230V_M-Bus_187F8309" (IFCIDENTIFIER)
  Danfoss | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Body Material = "Danfoss Plastic White" (IFCLABEL)
    Description = "Energy Calculator" (IFCTEXT)
    Energy Unit = "1 kWh" (IFCTEXT)
    H = 61. (IFCLENGTHMEASURE) [MILLI METRE]
    IfcExportAs = "IfcValveType" (IFCTEXT)
    IfcExportType = "Supercal 5" (IFCTEXT)
    Installation = "Return" (IFCTEXT)
    Interface Module = "No interface module" (IFCTEXT)
    Intergrated Communication = "M-Bus" (IFCTEXT)
    L = 143. (IFCLENGTHMEASURE) [MILLI METRE]
    LOD 200 = FALSE (IFCBOOLEAN)
    LOD 350 = TRUE (IFCBOOLEAN)
    Manufacturer = "Danfoss" (IFCTEXT)
    Max Diameter = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Max Flow (Text) = "25 m³/h" (IFCTEXT)
    Max Flow = 6.9444444444444429 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Max Medium Temperature = "55 °C" (IFCTEXT)
    Min Diameter = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Min Flow = "6 m³/h" (IFCTEXT)
    Min Medium Temperature = "5 °C" (IFCTEXT)
    Model = "187F8309" (IFCTEXT)
    Model Type = "Supercal 5_1l/p_230V_M-Bus" (IFCTEXT)
    Pulse Value Volume = "1 l/pulse" (IFCTEXT)
    Supply Voltage Type = "mains unit" (IFCTEXT)
    URL = "https://store.danfoss.com/en/Climate-Solutions-for-heating/Energy-meters/Calculators/c/6953?q=%3Arelevance%3Adanfoss_producttypehierarchydesc%3ASupercal+5&text=" (IFCTEXT)
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    W = 158.00000000000003 (IFCLENGTHMEASURE) [MILLI METRE]
    Weight = 0.63 (IFCMASSMEASURE) [KILO GRAM]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Danfoss" (IFCLABEL)